element SignalPdu

diagram |
type | extension of X3DNetworkSensorNode
properties |
content | complex
children | IS MetadataBoolean MetadataDouble MetadataFloat MetadataInteger MetadataSet MetadataString
used by |
element | TransformSensor
groups | ChildContentModelDIS PickSensorGroupingNodeContentModel
attributes |
Name | Type | Use | Default | Fixed | Annotation
DEF | xs:ID |  |  |  |
appinfo
DEF defines a unique ID name for each node, referenceable by other nodes.
USE | xs:IDREF |  |  |  |
appinfo
USE means reuse an already DEF-ed node ID, excluding all child nodes and all other attributes (except for containerField, which can have a different value).
class | xs:NMTOKENS |  |  |  |
appinfo
The class attribute is a space-separated list of classes, reserved for use by Cascading Style Sheets (CSS) and XML stylesheets. This attribute is only functional if the X3D model is loaded within an HTML page.
id | xs:NMTOKEN |  |  |  |
appinfo
The id attribute is a unique identifier, reserved for use by HTML5/DOM pages, independent of DEF labeling and internal X3D node referencing. This attribute is only functional if the X3D model is loaded within an HTML page.
style | SFString |  |  |  |
appinfo
The style attribute provides an inline block of CSS for element styling, reserved for use by Cascading Style Sheets (CSS) and XML stylesheets. This attribute is only functional if the X3D model is loaded within an HTML page.
description | SFString |  |  |  |
enabled | SFBool |  | true |  |
bboxCenter | SFVec3f |  | 0 0 0 |  |
bboxSize | bboxSizeType |  | -1 -1 -1 |  |
bboxDisplay | SFBool |  | false |  |
visible | SFBool |  | true |  |
whichGeometry | SFInt32 |  | 1 |  |
readInterval | derived by: SFTime |  | 0.1 |  |
writeInterval | derived by: SFTime |  | 1.0 |  |
networkMode | networkModeChoices |  | standAlone |  |
siteID | SFInt32 |  | 0 |  |
applicationID | SFInt32 |  | 0 |  |
entityID | SFInt32 |  | 0 |  |
address | SFString |  | localhost |  |
port | SFInt32 |  | 0 |  |
multicastRelayHost | SFString |  |  |  |
multicastRelayPort | SFInt32 |  | 0 |  |
rtpHeaderExpected | SFBool |  | false |  |
radioID | SFInt32 |  | 0 |  |
encodingScheme | SFInt32 |  | 0 |  |
tdlType | SFInt32 |  | 0 |  |
sampleRate | SFInt32 |  | 0 |  |
samples | SFInt32 |  | 0 |  |
dataLength | SFInt32 |  | 0 |  |
data | MFInt32 |  |  |  |
geoSystem | geoSystemType |  | "GD" "WE" |  |
geoCoords | SFVec3d |  | 0 0 0 |  |
containerField | xs:NMTOKEN |  | children |  |
annotation |
appinfo
<xs:attribute name="isNetworkReader" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isNetworkWriter" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isRtpHeaderHeard" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isStandAlone" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="timestamp" fixed="outputOnlyField"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="additionalInterface" type="xs:string" default="X3DBoundedObject"/> <xs:attribute name="componentName" type="componentNameChoices" fixed="DIS"/> <xs:attribute name="componentLevel" type="xs:positiveInteger" fixed="1"/>
source | <xs:element name="SignalPdu"> <xs:annotation> <xs:appinfo> <xs:attribute name="isNetworkReader" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isNetworkWriter" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isRtpHeaderHeard" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isStandAlone" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="timestamp" fixed="outputOnlyField"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="additionalInterface" type="xs:string" default="X3DBoundedObject"/> <xs:attribute name="componentName" type="componentNameChoices" fixed="DIS"/> <xs:attribute name="componentLevel" type="xs:positiveInteger" fixed="1"/> </xs:appinfo> <xs:documentation source="https://www.web3d.org/specifications/X3Dv4/ISO-IEC19775-1v4-IS/Part01/components/dis.html#SignalPdu"/> </xs:annotation> <xs:complexType> <xs:complexContent> <xs:extension base="X3DNetworkSensorNode"> <xs:attribute name="bboxCenter" type="SFVec3f" default="0 0 0"/> <xs:attribute name="bboxSize" type="bboxSizeType" default="-1 -1 -1"/> <xs:attribute name="bboxDisplay" type="SFBool" default="false"/> <xs:attribute name="visible" type="SFBool" default="true"/> <xs:attribute name="whichGeometry" type="SFInt32" default="1"/> <xs:attribute name="readInterval" default="0.1"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="writeInterval" default="1.0"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="networkMode" type="networkModeChoices" default="standAlone"/> <xs:attribute name="siteID" type="SFInt32" default="0"/> <xs:attribute name="applicationID" type="SFInt32" default="0"/> <xs:attribute name="entityID" type="SFInt32" default="0"/> <xs:attribute name="address" type="SFString" default="localhost"/> <xs:attribute name="port" type="SFInt32" default="0"/> <xs:attribute name="multicastRelayHost" type="SFString"/> <xs:attribute name="multicastRelayPort" type="SFInt32" default="0"/> <xs:attribute name="rtpHeaderExpected" type="SFBool" default="false"/> <xs:attribute name="radioID" type="SFInt32" default="0"/> <xs:attribute name="encodingScheme" type="SFInt32" default="0"/> <xs:attribute name="tdlType" type="SFInt32" default="0"/> <xs:attribute name="sampleRate" type="SFInt32" default="0"/> <xs:attribute name="samples" type="SFInt32" default="0"/> <xs:attribute name="dataLength" type="SFInt32" default="0"/> <xs:attribute name="data" type="MFInt32"/> <xs:attribute name="geoSystem" type="geoSystemType" default='"GD" "WE"'/> <xs:attribute name="geoCoords" type="SFVec3d" default="0 0 0"/> <xs:attribute name="containerField" type="xs:NMTOKEN" default="children"/> </xs:extension> </xs:complexContent> </xs:complexType> </xs:element>

attribute SignalPdu/@bboxCenter

type | SFVec3f
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="bboxCenter" type="SFVec3f" default="0 0 0"/>

attribute SignalPdu/@bboxSize

type | bboxSizeType
properties |
default | -1 -1 -1
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*((([+]?(((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s*)|((\-1(\.(0)*)?([Ee][+-]?[0]+)?\s+){2}\-1(\.(0)*)?([Ee][+-]?[0]+)?)\s*)? |
source | <xs:attribute name="bboxSize" type="bboxSizeType" default="-1 -1 -1"/>

attribute SignalPdu/@bboxDisplay

type | SFBool
properties |
default | false
source | <xs:attribute name="bboxDisplay" type="SFBool" default="false"/>

attribute SignalPdu/@visible

type | SFBool
properties |
default | true
source | <xs:attribute name="visible" type="SFBool" default="true"/>

attribute SignalPdu/@whichGeometry

type | SFInt32
properties |
default | 1
source | <xs:attribute name="whichGeometry" type="SFInt32" default="1"/>

attribute SignalPdu/@readInterval

type | restriction of SFTime
properties |
default | 0.1
facets |
Kind | Value | Annotation
minInclusive | 0 |
source | <xs:attribute name="readInterval" default="0.1"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute>

attribute SignalPdu/@writeInterval

type | restriction of SFTime
properties |
default | 1.0
facets |
Kind | Value | Annotation
minInclusive | 0 |
source | <xs:attribute name="writeInterval" default="1.0"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute>

attribute SignalPdu/@networkMode

type | networkModeChoices
properties |
default | standAlone
facets |
Kind | Value | Annotation
enumeration | standAlone |
appinfo
ignore network but still respond to events in local scene
enumeration | networkReader |
appinfo
listen to network and read PDU packets at readInterval, act as remotely linked copy of entity
enumeration | networkWriter |
appinfo
send PDU packets to network at writeInterval, act as master entity
source | <xs:attribute name="networkMode" type="networkModeChoices" default="standAlone"/>

attribute SignalPdu/@siteID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="siteID" type="SFInt32" default="0"/>

attribute SignalPdu/@applicationID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="applicationID" type="SFInt32" default="0"/>

attribute SignalPdu/@entityID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="entityID" type="SFInt32" default="0"/>

attribute SignalPdu/@address

type | SFString
properties |
default | localhost
source | <xs:attribute name="address" type="SFString" default="localhost"/>

attribute SignalPdu/@port

type | SFInt32
properties |
default | 0
source | <xs:attribute name="port" type="SFInt32" default="0"/>

attribute SignalPdu/@multicastRelayHost

type | SFString
source | <xs:attribute name="multicastRelayHost" type="SFString"/>

attribute SignalPdu/@multicastRelayPort

type | SFInt32
properties |
default | 0
source | <xs:attribute name="multicastRelayPort" type="SFInt32" default="0"/>

attribute SignalPdu/@rtpHeaderExpected

type | SFBool
properties |
default | false
source | <xs:attribute name="rtpHeaderExpected" type="SFBool" default="false"/>

attribute SignalPdu/@radioID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioID" type="SFInt32" default="0"/>

attribute SignalPdu/@encodingScheme

type | SFInt32
properties |
default | 0
source | <xs:attribute name="encodingScheme" type="SFInt32" default="0"/>

attribute SignalPdu/@tdlType

type | SFInt32
properties |
default | 0
source | <xs:attribute name="tdlType" type="SFInt32" default="0"/>

attribute SignalPdu/@sampleRate

type | SFInt32
properties |
default | 0
source | <xs:attribute name="sampleRate" type="SFInt32" default="0"/>

attribute SignalPdu/@samples

type | SFInt32
properties |
default | 0
source | <xs:attribute name="samples" type="SFInt32" default="0"/>

attribute SignalPdu/@dataLength

type | SFInt32
properties |
default | 0
source | <xs:attribute name="dataLength" type="SFInt32" default="0"/>

attribute SignalPdu/@data

type | MFInt32
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*([+-]?(0|[1-9][0-9]*)([Ee][+-]?[0-9]+)?\s*,?\s*)* |
source | <xs:attribute name="data" type="MFInt32"/>

attribute SignalPdu/@geoSystem

type | geoSystemType
properties |
default | "GD" "WE"
source | <xs:attribute name="geoSystem" type="geoSystemType" default='"GD" "WE"'/>

attribute SignalPdu/@geoCoords

type | SFVec3d
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="geoCoords" type="SFVec3d" default="0 0 0"/>

attribute SignalPdu/@containerField

type | xs:NMTOKEN
properties |
default | children
source | <xs:attribute name="containerField" type="xs:NMTOKEN" default="children"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy