element TransmitterPdu

diagram |
type | extension of X3DNetworkSensorNode
properties |
content | complex
children | IS MetadataBoolean MetadataDouble MetadataFloat MetadataInteger MetadataSet MetadataString
used by |
element | TransformSensor
groups | ChildContentModelDIS PickSensorGroupingNodeContentModel
attributes |
Name | Type | Use | Default | Fixed | Annotation
DEF | xs:ID |  |  |  |
appinfo
DEF defines a unique ID name for each node, referenceable by other nodes.
USE | xs:IDREF |  |  |  |
appinfo
USE means reuse an already DEF-ed node ID, excluding all child nodes and all other attributes (except for containerField, which can have a different value).
class | xs:NMTOKENS |  |  |  |
appinfo
The class attribute is a space-separated list of classes, reserved for use by Cascading Style Sheets (CSS) and XML stylesheets. This attribute is only functional if the X3D model is loaded within an HTML page.
id | xs:NMTOKEN |  |  |  |
appinfo
The id attribute is a unique identifier, reserved for use by HTML5/DOM pages, independent of DEF labeling and internal X3D node referencing. This attribute is only functional if the X3D model is loaded within an HTML page.
style | SFString |  |  |  |
appinfo
The style attribute provides an inline block of CSS for element styling, reserved for use by Cascading Style Sheets (CSS) and XML stylesheets. This attribute is only functional if the X3D model is loaded within an HTML page.
description | SFString |  |  |  |
enabled | SFBool |  | true |  |
bboxCenter | SFVec3f |  | 0 0 0 |  |
bboxSize | bboxSizeType |  | -1 -1 -1 |  |
bboxDisplay | SFBool |  | false |  |
visible | SFBool |  | true |  |
whichGeometry | SFInt32 |  | 1 |  |
readInterval | derived by: SFTime |  | 0.1 |  |
writeInterval | derived by: SFTime |  | 1.0 |  |
networkMode | networkModeChoices |  | standAlone |  |
siteID | SFInt32 |  | 0 |  |
applicationID | SFInt32 |  | 0 |  |
entityID | SFInt32 |  | 0 |  |
address | SFString |  | localhost |  |
port | SFInt32 |  | 0 |  |
multicastRelayHost | SFString |  |  |  |
multicastRelayPort | SFInt32 |  | 0 |  |
rtpHeaderExpected | SFBool |  | false |  |
radioID | SFInt32 |  | 0 |  |
antennaLocation | SFVec3f |  | 0 0 0 |  |
antennaPatternLength | SFInt32 |  | 0 |  |
antennaPatternType | SFInt32 |  | 0 |  |
cryptoKeyID | SFInt32 |  | 0 |  |
cryptoSystem | SFInt32 |  | 0 |  |
frequency | derived by: SFInt32 |  | 0 |  |
inputSource | SFInt32 |  | 0 |  |
lengthOfModulationParameters | SFInt32 |  | 0 |  |
modulationTypeDetail | SFInt32 |  | 0 |  |
modulationTypeMajor | SFInt32 |  | 0 |  |
modulationTypeSpreadSpectrum | SFInt32 |  | 0 |  |
modulationTypeSystem | SFInt32 |  | 0 |  |
power | SFFloat |  | 0.0 |  |
radioEntityTypeCategory | SFInt32 |  | 0 |  |
radioEntityTypeCountry | SFInt32 |  | 0 |  |
radioEntityTypeDomain | SFInt32 |  | 0 |  |
radioEntityTypeKind | SFInt32 |  | 0 |  |
radioEntityTypeNomenclature | SFInt32 |  | 0 |  |
radioEntityTypeNomenclatureVersion | SFInt32 |  | 0 |  |
relativeAntennaLocation | SFVec3f |  | 0 0 0 |  |
transmitFrequencyBandwidth | SFFloat |  | 0 |  |
transmitState | SFInt32 |  | 0 |  |
geoSystem | geoSystemType |  | "GD" "WE" |  |
geoCoords | SFVec3d |  | 0 0 0 |  |
containerField | xs:NMTOKEN |  | children |  |
annotation |
appinfo
<xs:attribute name="isNetworkReader" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isNetworkWriter" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isRtpHeaderHeard" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isStandAlone" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="timestamp" fixed="outputOnlyField"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="additionalInterface" type="xs:string" default="X3DBoundedObject"/> <xs:attribute name="componentName" type="componentNameChoices" fixed="DIS"/> <xs:attribute name="componentLevel" type="xs:positiveInteger" fixed="1"/>
source | <xs:element name="TransmitterPdu"> <xs:annotation> <xs:appinfo> <xs:attribute name="isNetworkReader" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isNetworkWriter" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isRtpHeaderHeard" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isStandAlone" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="timestamp" fixed="outputOnlyField"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="additionalInterface" type="xs:string" default="X3DBoundedObject"/> <xs:attribute name="componentName" type="componentNameChoices" fixed="DIS"/> <xs:attribute name="componentLevel" type="xs:positiveInteger" fixed="1"/> </xs:appinfo> <xs:documentation source="https://www.web3d.org/specifications/X3Dv4/ISO-IEC19775-1v4-IS/Part01/components/dis.html#TransmitterPdu"/> </xs:annotation> <xs:complexType> <xs:complexContent> <xs:extension base="X3DNetworkSensorNode"> <xs:attribute name="bboxCenter" type="SFVec3f" default="0 0 0"/> <xs:attribute name="bboxSize" type="bboxSizeType" default="-1 -1 -1"/> <xs:attribute name="bboxDisplay" type="SFBool" default="false"/> <xs:attribute name="visible" type="SFBool" default="true"/> <xs:attribute name="whichGeometry" type="SFInt32" default="1"/> <xs:attribute name="readInterval" default="0.1"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="writeInterval" default="1.0"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="networkMode" type="networkModeChoices" default="standAlone"/> <xs:attribute name="siteID" type="SFInt32" default="0"/> <xs:attribute name="applicationID" type="SFInt32" default="0"/> <xs:attribute name="entityID" type="SFInt32" default="0"/> <xs:attribute name="address" type="SFString" default="localhost"/> <xs:attribute name="port" type="SFInt32" default="0"/> <xs:attribute name="multicastRelayHost" type="SFString"/> <xs:attribute name="multicastRelayPort" type="SFInt32" default="0"/> <xs:attribute name="rtpHeaderExpected" type="SFBool" default="false"/> <xs:attribute name="radioID" type="SFInt32" default="0"/> <xs:attribute name="antennaLocation" type="SFVec3f" default="0 0 0"/> <xs:attribute name="antennaPatternLength" type="SFInt32" default="0"/> <xs:attribute name="antennaPatternType" type="SFInt32" default="0"/> <xs:attribute name="cryptoKeyID" type="SFInt32" default="0"/> <xs:attribute name="cryptoSystem" type="SFInt32" default="0"/> <xs:attribute name="frequency" default="0"> <xs:simpleType> <xs:restriction base="SFInt32"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="inputSource" type="SFInt32" default="0"/> <xs:attribute name="lengthOfModulationParameters" type="SFInt32" default="0"/> <xs:attribute name="modulationTypeDetail" type="SFInt32" default="0"/> <xs:attribute name="modulationTypeMajor" type="SFInt32" default="0"/> <xs:attribute name="modulationTypeSpreadSpectrum" type="SFInt32" default="0"/> <xs:attribute name="modulationTypeSystem" type="SFInt32" default="0"/> <xs:attribute name="power" type="SFFloat" default="0.0"/> <xs:attribute name="radioEntityTypeCategory" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeCountry" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeDomain" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeKind" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeNomenclature" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeNomenclatureVersion" type="SFInt32" default="0"/> <xs:attribute name="relativeAntennaLocation" type="SFVec3f" default="0 0 0"/> <xs:attribute name="transmitFrequencyBandwidth" type="SFFloat" default="0"/> <xs:attribute name="transmitState" type="SFInt32" default="0"/> <xs:attribute name="geoSystem" type="geoSystemType" default='"GD" "WE"'/> <xs:attribute name="geoCoords" type="SFVec3d" default="0 0 0"/> <xs:attribute name="containerField" type="xs:NMTOKEN" default="children"/> </xs:extension> </xs:complexContent> </xs:complexType> </xs:element>

attribute TransmitterPdu/@bboxCenter

type | SFVec3f
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="bboxCenter" type="SFVec3f" default="0 0 0"/>

attribute TransmitterPdu/@bboxSize

type | bboxSizeType
properties |
default | -1 -1 -1
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*((([+]?(((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s*)|((\-1(\.(0)*)?([Ee][+-]?[0]+)?\s+){2}\-1(\.(0)*)?([Ee][+-]?[0]+)?)\s*)? |
source | <xs:attribute name="bboxSize" type="bboxSizeType" default="-1 -1 -1"/>

attribute TransmitterPdu/@bboxDisplay

type | SFBool
properties |
default | false
source | <xs:attribute name="bboxDisplay" type="SFBool" default="false"/>

attribute TransmitterPdu/@visible

type | SFBool
properties |
default | true
source | <xs:attribute name="visible" type="SFBool" default="true"/>

attribute TransmitterPdu/@whichGeometry

type | SFInt32
properties |
default | 1
source | <xs:attribute name="whichGeometry" type="SFInt32" default="1"/>

attribute TransmitterPdu/@readInterval

type | restriction of SFTime
properties |
default | 0.1
facets |
Kind | Value | Annotation
minInclusive | 0 |
source | <xs:attribute name="readInterval" default="0.1"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute>

attribute TransmitterPdu/@writeInterval

type | restriction of SFTime
properties |
default | 1.0
facets |
Kind | Value | Annotation
minInclusive | 0 |
source | <xs:attribute name="writeInterval" default="1.0"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute>

attribute TransmitterPdu/@networkMode

type | networkModeChoices
properties |
default | standAlone
facets |
Kind | Value | Annotation
enumeration | standAlone |
appinfo
ignore network but still respond to events in local scene
enumeration | networkReader |
appinfo
listen to network and read PDU packets at readInterval, act as remotely linked copy of entity
enumeration | networkWriter |
appinfo
send PDU packets to network at writeInterval, act as master entity
source | <xs:attribute name="networkMode" type="networkModeChoices" default="standAlone"/>

attribute TransmitterPdu/@siteID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="siteID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@applicationID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="applicationID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@entityID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="entityID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@address

type | SFString
properties |
default | localhost
source | <xs:attribute name="address" type="SFString" default="localhost"/>

attribute TransmitterPdu/@port

type | SFInt32
properties |
default | 0
source | <xs:attribute name="port" type="SFInt32" default="0"/>

attribute TransmitterPdu/@multicastRelayHost

type | SFString
source | <xs:attribute name="multicastRelayHost" type="SFString"/>

attribute TransmitterPdu/@multicastRelayPort

type | SFInt32
properties |
default | 0
source | <xs:attribute name="multicastRelayPort" type="SFInt32" default="0"/>

attribute TransmitterPdu/@rtpHeaderExpected

type | SFBool
properties |
default | false
source | <xs:attribute name="rtpHeaderExpected" type="SFBool" default="false"/>

attribute TransmitterPdu/@radioID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@antennaLocation

type | SFVec3f
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="antennaLocation" type="SFVec3f" default="0 0 0"/>

attribute TransmitterPdu/@antennaPatternLength

type | SFInt32
properties |
default | 0
source | <xs:attribute name="antennaPatternLength" type="SFInt32" default="0"/>

attribute TransmitterPdu/@antennaPatternType

type | SFInt32
properties |
default | 0
source | <xs:attribute name="antennaPatternType" type="SFInt32" default="0"/>

attribute TransmitterPdu/@cryptoKeyID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="cryptoKeyID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@cryptoSystem

type | SFInt32
properties |
default | 0
source | <xs:attribute name="cryptoSystem" type="SFInt32" default="0"/>

attribute TransmitterPdu/@frequency

type | restriction of SFInt32
properties |
default | 0
facets |
Kind | Value | Annotation
minInclusive | 0 |
source | <xs:attribute name="frequency" default="0"> <xs:simpleType> <xs:restriction base="SFInt32"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute>

attribute TransmitterPdu/@inputSource

type | SFInt32
properties |
default | 0
source | <xs:attribute name="inputSource" type="SFInt32" default="0"/>

attribute TransmitterPdu/@lengthOfModulationParameters

type | SFInt32
properties |
default | 0
source | <xs:attribute name="lengthOfModulationParameters" type="SFInt32" default="0"/>

attribute TransmitterPdu/@modulationTypeDetail

type | SFInt32
properties |
default | 0
source | <xs:attribute name="modulationTypeDetail" type="SFInt32" default="0"/>

attribute TransmitterPdu/@modulationTypeMajor

type | SFInt32
properties |
default | 0
source | <xs:attribute name="modulationTypeMajor" type="SFInt32" default="0"/>

attribute TransmitterPdu/@modulationTypeSpreadSpectrum

type | SFInt32
properties |
default | 0
source | <xs:attribute name="modulationTypeSpreadSpectrum" type="SFInt32" default="0"/>

attribute TransmitterPdu/@modulationTypeSystem

type | SFInt32
properties |
default | 0
source | <xs:attribute name="modulationTypeSystem" type="SFInt32" default="0"/>

attribute TransmitterPdu/@power

type | SFFloat
properties |
default | 0.0
facets |
Kind | Value | Annotation
pattern | \s*([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="power" type="SFFloat" default="0.0"/>

attribute TransmitterPdu/@radioEntityTypeCategory

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeCategory" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeCountry

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeCountry" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeDomain

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeDomain" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeKind

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeKind" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeNomenclature

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeNomenclature" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeNomenclatureVersion

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeNomenclatureVersion" type="SFInt32" default="0"/>

attribute TransmitterPdu/@relativeAntennaLocation

type | SFVec3f
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="relativeAntennaLocation" type="SFVec3f" default="0 0 0"/>

attribute TransmitterPdu/@transmitFrequencyBandwidth

type | SFFloat
properties |
default | 0
facets |
Kind | Value | Annotation
pattern | \s*([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="transmitFrequencyBandwidth" type="SFFloat" default="0"/>

attribute TransmitterPdu/@transmitState

type | SFInt32
properties |
default | 0
source | <xs:attribute name="transmitState" type="SFInt32" default="0"/>

attribute TransmitterPdu/@geoSystem

type | geoSystemType
properties |
default | "GD" "WE"
source | <xs:attribute name="geoSystem" type="geoSystemType" default='"GD" "WE"'/>

attribute TransmitterPdu/@geoCoords

type | SFVec3d
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="geoCoords" type="SFVec3d" default="0 0 0"/>

attribute TransmitterPdu/@containerField

type | xs:NMTOKEN
properties |
default | children
source | <xs:attribute name="containerField" type="xs:NMTOKEN" default="children"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy