simpleType appliedParametersChoices

type | restriction of MFString
properties |
base | MFString
facets |
Kind | Value | Annotation
enumeration | "BOUNCE" |
appinfo
The bounce field value is used.
enumeration | "USER_FRICTION" |
appinfo
The system will normally calculate the friction direction vector that is perpendicular to the contact normal. This setting indicates that the user-supplied value in this contact should be used.
enumeration | "FRICTION_COEFFICIENT-2" |
appinfo
Apply frictionCoefficients values
enumeration | "ERROR_REDUCTION" |
appinfo
Apply softnessErrorCorrection value
enumeration | "CONSTANT_FORCE" |
appinfo
Apply softnessConstantForceMix value
enumeration | "SPEED-1" |
appinfo
Apply first component of surfaceSpeed array
enumeration | "SPEED-2" |
appinfo
Apply second component of surfaceSpeed array
enumeration | "SLIP-1" |
appinfo
Apply first component of slipFactors array
enumeration | "SLIP-2" |
appinfo
Apply second component of slipFactors array
annotation |
appinfo
Default global parameters for collision outputs of rigid body physics system. Contact node can override parent CollisionCollection node. Multiple optional values, but appliedParameters enumerations cannot be extended.
source | <xs:simpleType name="appliedParametersChoices"> <xs:annotation> <xs:appinfo>Default global parameters for collision outputs of rigid body physics system. Contact node can override parent CollisionCollection node. Multiple optional values, but appliedParameters enumerations cannot be extended.</xs:appinfo> <!-- Note that strict validation does not occur via schema since MFString allows any value. --> <xs:documentation source="https://www.web3d.org/documents/specifications/19775-1/V3.3/Part01/components/rigid_physics.html#t-AppliedParametersValidValues"/> </xs:annotation> <xs:restriction base="MFString"> <xs:enumeration value='"BOUNCE"'> <xs:annotation> <xs:appinfo>The bounce field value is used.</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value='"USER_FRICTION"'> <xs:annotation> <xs:appinfo>The system will normally calculate the friction direction vector that is perpendicular to the contact normal. This setting indicates that the user-supplied value in this contact should be used.</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value='"FRICTION_COEFFICIENT-2"'> <xs:annotation> <xs:appinfo>Apply frictionCoefficients values</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value='"ERROR_REDUCTION"'> <xs:annotation> <xs:appinfo>Apply softnessErrorCorrection value</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value='"CONSTANT_FORCE"'> <xs:annotation> <xs:appinfo>Apply softnessConstantForceMix value</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value='"SPEED-1"'> <xs:annotation> <xs:appinfo>Apply first component of surfaceSpeed array</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value='"SPEED-2"'> <xs:annotation> <xs:appinfo>Apply second component of surfaceSpeed array</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value='"SLIP-1"'> <xs:annotation> <xs:appinfo>Apply first component of slipFactors array</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value='"SLIP-2"'> <xs:annotation> <xs:appinfo>Apply second component of slipFactors array</xs:appinfo> </xs:annotation> </xs:enumeration> </xs:restriction> </xs:simpleType>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy